For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel (I/P) defroster grille. Refer to Defroster Grille Replacement.
2. Remove the screws (1) securing the speaker to the I/P.
3. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connector.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the screws (1) securing the speaker to the I/P.

Tighten
Tighten the screws (1) to 2 N·m (18 lb in).

3. Install the instrument panel defroster grille. Refer to Defroster Grille Replacement.