For 1990-2009 cars

Icon | Icon Definition
--- | ---
| Notice: The OBD II symbol is used on the circuit diagrams in order to alert the technician that the circuit is essential for proper OBD II emission control circuit operation. Any circuit which fails and causes the malfunction indicator lamp (MIL) to turn ON, or causes emissions-related component damage, is identified as an OBD II circuit.
| Important: Twisted-pair wires provide an effective shield that helps protect sensitive electronic components from electrical interference. If the wires were covered with shielding, install new shielding. In order to prevent electrical interference from degrading the performance of the connected components, you must maintain the proper specification when making any repairs to the twisted-pair wires shown :

• | The wires must be twisted a minimum of 9 turns per 31 cm (12 in) as measured anywhere along the length of the wires.

• | The outside diameter of the twisted wires must not exceed 6.0 mm (0.25 in).