For 1990-2009 cars

### Removal Procedure

1. Use a flat-bladed tool in order to remove the speaker grille.
2. Remove the screws securing the speaker to the seat.
3. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connectors.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the screws securing the speaker to the seat.

Tighten
Tighten the screws to 2 N·m (18 lb in).

3. Install the speaker grille.