For 1990-2009 cars

#### Special Tools

J 38778 Door Trim Pad Clip Remover

### Removal Procedure

1. Use a J 38778 to release the retainer clips from the rocker panel.
2. Remove the front carpet retainer.

### Installation Procedure

1. Align the front carpet retainer with the slots in the rocker panel.
2. Apply pressure along the entire length of the molding in order to secure the retainers.
3. Ensure the fit at the lower center pillar garnish molding is secure to the front carpet retainer.