For 1990-2009 cars

## Instrument Panel Air Outlet Ducts Replacement Upper Left

### Removal Procedure

1. Remove the instrument panel (I/P) retainer. Refer to Instrument Panel Carrier Replacement.
2. Remove the foam dash pad (1).
3. Remove the screws (1) that retain the air duct.
4. Remove the left air duct (2) by unsnapping the air duct from the HVAC module.

### Installation Procedure

1. Install the left air duct (2) by pressing down until you hear the tabs engage on the HVAC module.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the air outlet duct screws (1).

Tighten
Tighten the screws to 2 N·m (18 lb in).

3. Install the foam dash pad (1).
4. Install the I/P retainer. Refer to Instrument Panel Carrier Replacement.

## Instrument Panel Air Outlet Ducts Replacement Upper Right

### Removal Procedure

1. Remove the instrument panel (I/P) retainer. Refer to Instrument Panel Carrier Replacement.
2. Remove the foam dash pad (1).
3. Remove the screws (1) that retain the air duct (2).
4. Remove the right air duct (2) by releasing the tabs from the module.

### Installation Procedure

1. Install the right air duct (2) by pressing down until you hear the tabs engage on the HVAC module.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the right air duct screws (1).

Tighten
Tighten the screws to 2 N·m (18 lb in).

3. Install the foam dash pad (1).
4. Install the I/P retainer. Refer to Instrument Panel Carrier Replacement.