For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Prop Shaft Trans Flange
2 | NEW Front Prop Shaft Flange Nut Notice: Refer to Fastener Notice in the Preface section. Tighten Tighten the nut to 105 N·m (77 lb ft).

#### Special Tools

J 45012 Holding Fixture

3 | Output Shaft Notice: Stake the flange nut onto the output shaft. Use the two staking grooves on the shaft to locate the staking points. Failure to stake the flange nut may result in damage to the transmission.