For 1990-2009 cars

Table 1: | Driver Door Module (DDM)
Table 2: | ECM - 4.6L (LH2), 3.6L (LY7)
Table 3: | IPM
Table 4: | LRDM
Table 5: | PDM
Table 6: | RCDLR
Table 7: | Rear Integration Module (RIM)
Table 8: | RRDM

#### Driver Door Module (DDM)

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Operating Conditions: Ignition ON, Engine OFF.
Door Ajar Switch | Data | Door Closed/Ajar | Door Closed
VIN Learned | VIN Information | Yes/No | Yes
VIN Information Received | VIN Information | Yes/No | Yes

#### ECM - 4.6L (LH2), 3.6L (LY7)

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Operating Conditions: Ignition ON, Engine OFF.
VTD Password Learn Enabled | Electrical/Theft Data | Yes/No | No
Vehicle Security Status | Data | Fuel Continue/Fuel Lockout/Fuel Disabled/Learn Timer Active/Fail Enable/Learn Enable | Fuel Continue
VTD Fuel Disable | Electrical/Theft Data | Active/Inactive | Inactive
Automatic VTD Learn Timer | Electrical/Theft Data | Active/Inactive | Inactive
VTD Fuel Disable Until Ignition Off | Electrical/Theft Data | Yes/No | No
VTD Fuel Enabled | Electrical/Theft Data | Yes/No | No
ECM in VTD Fail Enable | Electrical/Theft Data | Yes/No | No

#### IPM

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Operating Conditions: Ignition ON, Engine OFF.
Valet Switch | Input Signal | Active/Inactive | Inactive

#### LRDM

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Operating Conditions: Ignition ON, Engine OFF.
Door Ajar Switch | Data | Door Closed/Ajar | Door Closed
Learned VIN | VIN Information | Yes/No | Yes
VIN Information Received | VIN Information | Yes/No | Yes

#### PDM

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Operating Conditions: Ignition ON, Engine OFF.
Door Ajar Switch | Data | Door Closed/Ajar | Door Closed
Learned VIN | VIN Information | Yes/No | Yes
VIN Information Received | VIN Information | Yes/No | Yes

#### RCDLR

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Operating Conditions: Ignition ON, Engine OFF.
Battery Reconnected | Substitution Detection | Yes/No | No
DDM Substitution | Substitution Detection | Unknown/Yes/No | No
DPM Substitution | Substitution Detection | Unknown/Yes/No | No
IPC Substitution | Substitution Detection | Unknown/Yes/No | No
LRDM Substitution | Substitution Detection | Unknown/Yes/No | No
PDM Substitution | Substitution Detection | Unknown/Yes/No | No
RIM Substitution | Substitution Detection | Unknown/Yes/No | No
RRDM Substitution | Substitution Detection | Unknown/Yes/No | No
Substitution Detection Status | Substitution Detection | Pass/Fail | Pass
Backfire Signal | Substitution Detection | On/Off | Off
Valid RCDLR VIN | Substitution Detection | Yes/No | No

#### Rear Integration Module (RIM)

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Operating Conditions: Ignition ON, Engine OFF.
CTD Status | CTD: Information | Disabled/Disarmed/Alarm Inhibit/Arming/Armed/Alarm | Disabled
Hood Closed Switch | Input Signal | Active/Inactive | Active
Hood Open Switch | Input Signal | Active/Inactive | Inactive
Tilt Sensor | Input Signal | Active/Inactive | Inactive
Tilt Sensor Status | CTD: Information | Valid/Invalid | Valid
Tilt Sensor Enable | CTD: Information | Yes/No | No
Intrusion Sensor | Input Signal | Active/Inactive | Inactive
Intrusion Sensor Status | CTD: Information | Valid/Invalid | Valid
Intrusion Sensor Enable | CTD: Information | Yes/No | No
Trunk Lid Ajar | Input Signal | Closed/Ajar | Ajar
Anti-theft Alarm Status | CTD: Information | Disarm/Armed/Blip/Alarm | Removal
Triggers Per Theft Cycle | CTD: Information | Number | Varies
Engine Hood Ajar | Alarm Triggers | Yes/No | No
Trunk Lid Ajar | Alarm Triggers | Yes/No | No
Battery Disconnected | Alarm Triggers | Yes/No | No
Left Front Door Ajar Switch | Alarm Triggers | Yes/No | No
Right Front Door Ajar Switch | Alarm Triggers | Yes/No | No
Door Jamb Switch - Left Rear | Alarm Triggers | Yes/No | No
Door Jamb Switch - Right Rear | Alarm Triggers | Yes/No | No
Intrusion Sensor | Alarm Triggers | Yes/No | No
Tilt Sensor | Alarm Triggers | Yes/No | No

#### RRDM

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Operating Conditions: Ignition ON, Engine OFF.
Door Ajar Switch | Data | Door Closed/Ajar | Door Closed
Learned VIN | VIN Information | Yes/No | Yes
VIN Information Received | VIN Information | Yes/No | Yes