For 1990-2009 cars

#### Special Tools

• | EN-46103 Camshaft Actuator Valve Seal Remover/Installer

• | J 29184 Oil Seal Installer

Important: Do not lubricate the crankshaft front oil seal or crankshaft balancer sealing surfaces. The crankshaft balancer is installed into a dry seal.

1. Install the NEW crankshaft front oil seal into the engine front cover using the J 29184 .
2. Place the seal into position with the notches (1) in the seal down. The notches (1) will face inboard when properly installed.
3. Install the NEW camshaft position actuator valve oil seals into the engine front cover using the EN-46103 .