For 1990-2009 cars

### Removal Procedure

1. Remove the cupholder from the bridge console. Refer to Cupholder Replacement.
2. Remove the bolts securing the rear of the bridge console to the bezel.
3. Remove the bezel from the bridge console.

### Installation Procedure

1. Install the bezel to the bridge console.
2. Install the bolts securing the bezel to the bridge console.
3. Install the cupholder to the bridge console. Refer to Cupholder Replacement.