For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the tires and wheel. Refer to Tire and Wheel Removal and Installation.
3. Remove inner stabilizer shaft link to stabilizer shaft retaining nut.
4. Separate the stabilizer shaft link from the stabilizer shaft.
5. Remove the stabilizer shaft bracket mounting bolts.
6. Remove the stabilizer shaft bracket.
7. Remove the stabilizer shaft insulator.

### Installation Procedure

1. Install the stabilizer shaft insulator to the stabilizer shaft with the slit facing rearward.
2. Install the stabilizer shaft bracket.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the stabilizer shaft bracket mounting bolts.

Tighten
Tighten the bolts to 110 N·m (81 lb ft).

4. Install the stabilizer shaft link to the stabilizer shaft.
5. Install stabilizer shaft link to stabilizer shaft retaining nut.

Tighten
Tighten the nut to 115 N·m (85 lb ft).

6. Install the tire and wheel. Refer to Tire and Wheel Removal and Installation.
7. Lower the vehicle.