For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel retainer. Refer to Instrument Panel Assembly Replacement .
2. Remove the fasteners securing the global position antenna to the I/P.
3. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connector.
2. Install the fasteners securing the antenna to I/P.
3. Install the instrument panel retainers. Refer to Instrument Panel Assembly Replacement .