For 1990-2009 cars

Note: Complete the left and right rear toe adjustments separately, per wheel. Using the following procedure.

1. Loosen the adjustment link jam nuts (1).
2. In order to adjust the toe, rotate the turnbuckle (2).

Caution: Refer to Fastener Caution in the Preface section.

3. Hold the turnbuckle (2) when tightening the jam nuts (1).

Tighten
Tighten link nuts to 40 N·m (30 lb ft).

4. Re-check the toe setting after tightening.
5. Re-adjust the toe setting if necessary. Refer to Wheel Alignment Specifications.