For 1990-2009 cars

1. Install NEW O-rings on the evaporative emission (EVAP) purge valve and manifold absolute pressure (MAP) sensor.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the coolant fitting.

Tighten
Tighten the engine coolant air bleed fitting to 10 N·m (89 lb in).

3. Install the heater hose fitting.

Tighten
Tighten the heater hose fitting to 45 N·m (33 lb ft).

4. Install the NEW bypass hose.
5. Position the bypass hose clamp.
6. Install the MAP sensor.
7. Install the MAP sensor bolt.

Tighten
Tighten the MAP sensor bolt to 10 N·m (89 lb in).

8. Install the EVAP purge valve.
9. Install the EVAP purge valve bolt.

Tighten
Tighten the EVAP purge valve bolt to 10 N·m (89 lb in).

10. Install the intake manifold plenum duct.
11. Tighten the intake manifold plenum duct clamp.

Tighten
Tighten the intake manifold plenum duct clamp to 2.25 N·m (20 lb in).