For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat cushion. Refer to Rear Seat Cushion Cover and Pad Replacement.
2. Pry open cupholder bezel with a flat-bladed tool.
3. Loose the retainer from cushion back.
4. Remove the cupholder.

### Installation Procedure

1. Install the cupholder and bezel into the cushion.
2. Press inward with force, fasten the retainer.
3. Install the rear seat cushion. Refer to Rear Seat Cushion Cover and Pad Replacement.