For 1990-2009 cars

Callout | Component Name
--- | ---
Windshield Washer Pump Replacement

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation.
3. Remove the air deflector assembly. Refer to Front Air Deflector Replacement.

1 | Front Bumper Fascia Extension Trim Retainer (qty: 11)
2 | Front Bumper Fascia Extension Tip Right Hand only
3 | Wimndshield Washer Pump Assembly

1. Disconnect the washer hose and the bleeding washer solvent.
2. Disconnect the electrical connector.

4 | Windshield Washer Fluid Pump Lock Ring