For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Install the 1-2-3-4 and 3-5 reverse clutch housing with the 1-2-3-4 and 3-5 reverse clutch plates installed, onto the torque converter housing.
2. Install the DT 47868-2 onto the torque converter housing.
3. Install DT 47868-1 and DT-47868-3 onto the 3-5 reverse clutch backing plate.
4. Install the J 26900-13 onto DT 47868-2 .
5. Attach the J 8001 to the J 26900-13 and zero out the dial indicator on the DT 47868-1 .

#### Special Tools

• | DT 47868-1 Clutch Pack Travel Weight

• | DT 47868-2 Magnetic Base Adapter

• | DT-47868-3 Clutch Travel Weight Adapter (6L50 applications only)

• | J 8001 Dial Indicator Set

• | J 26900-13 Magnetic Base

1 | 3-5 Reverse Clutch Apply Passage Tip Apply compressed air to the apply passage hole, and observe the dial indicator measurement. Refer to Clutch Backing Plate Retaining Ring Specifications .