For 1990-2009 cars

Callout | Component Name
--- | ---

#### Front Bumper Impact Bar Assembly Replacement

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the air deflector. Refer to Front Air Deflector Replacement.

1 | Front Hood Retainer (Qty: 2)
2 | Front Hood Assembly
3 | Right Front Hood Retainer (Qty: 2)
4 | Right Front Hood Assembly
5 | Left Front Hood Retainer (Qty: 2)
6 | Left Front Hood Assembly
7 | Front Bumper Fascia Extension Locking Pin (Qty: 22)
8 | Front Bumper Fascia (Qty: 2)
9 | Front Bumper Fascia Side Lamp Electrical Connector Tip Remove and replace the front bumper fascia side and fog lamp electrical connector.
10 | Front Bumper Fascia Reinforcement Nut (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 9 N·m (80 lb in)
11 | Front Bumper Fascia Reinforcement Screw (Qty: 2) Tighten 9 N·m (80 lb in)
12 | Front Bumper Fascia Assembly Tip

• | Remove the retainers holding the fascia to the tie bar (Qty: 4)

• | If headlamp washer hose assembly is installed, disconnect it.

15 | Front Bumper Impact Bar Nut (Qty: 8) Tighten 25 N·m (18 lb ft)
16 | Front Bumper Impact Bar Assembly