For 1990-2009 cars

### Removal Procedure

1. Turn the ignition OFF.
2. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
3. Reposition the wiring harness heat shield to obtain access.
4. Disconnect the crankshaft position (CKP) electrical connector (3).
5. Remove the crankshaft sensor bolt.
6. Remove the crankshaft sensor.

### Installation Procedure

1. Install the crankshaft position sensor.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the crankshaft position sensor bolt and tighten to 10 N·m (89 lb in).
3. Connect the CKP electrical connector (3).
4. Install the wiring harness heat shield to the oil level indicator tube.
5. Lower the vehicle.