For 1990-2009 cars

#### Special Tools

J 37043 Park Brake Cable Release Tool

Caution: Refer to Brake Dust Caution in the Preface section.

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the rear tire and wheel assembly. Refer to Tire and Wheel Removal and Installation.
3. Pull down on the intermediate park brake cable (2) near the park brake cable connector (1).
4. Disconnect the intermediate park brake cable (2) from the park brake connector (1).
5. Use the J 37043 in order to depress the rear brake cable retainer.
6. Remove the rear park brake cable from the rear cable bracket (1).
7. Disconnect the park brake cable (2) from the park brake actuator lever (3).
8. Remove the park brake cable bracket mounting bolts.
9. Remove the park brake cable bracket.

### Installation Procedure

1. Install the park brake cable bracket.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the two park brake cable bracket mounting bolts.

Tighten
Tighten the park brake cable bracket mounting bolts to 60 N·m (44 lb ft).

3. Install the rear park brake cable (2) to the rear park brake cable bracket (1).
4. Ensure that the locking tabs are properly seated.
5. Connect the rear park brake cable (2) to the park brake actuator lever (3).
6. Pull down on the intermediate park brake cable (2) near the park brake cable connector (1).
7. Connect the intermediate park brake cable (2) to the park brake connector (1).
8. Install the rear tire and wheel assemblies. Refer to Tire and Wheel Removal and Installation.
9. Lower the vehicle.
10. To ensure that the park brake cable retainers are seated, cycle the park brake pedal 1 to 2 times.