For 1990-2009 cars

Callout | Part Name
--- | ---
1 | Hood Open Assist Rod Assembly Warning: Refer to Hood Hold-Open Device Warning in the Preface section. Caution: Refer to Liftgate Assist Rod Caution in the Preface section. Procedure Remove the metal clip at the ends of the assist rod, then pull away from stud.
2 | Hood Open Assist Rod Stud Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb in)
3 | Hood Open Assist Rod Stud Tighten 9 N·m (80 lb in)