For 1990-2009 cars

### Removal Procedure

1. Remove the oil pan. Refer to Oil Pan Replacement.
2. Remove the oil pan scraper bolts.
3. Remove the oil pan scraper.
4. Remove the oil suction pipe bolts.
5. Remove the oil suction pipe.
6. Remove the oil suction tube seal from the oil suction tube. Discard the oil suction tube seal.

### Installation Procedure

1. Install a NEW oil suction tube seal onto the oil suction tube. DO NOT reuse the old oil suction tube seal.
2. Install the oil suction pipe.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the oil suction pipe bolts.

Tighten
Tighten the oil suction pipe bolts to 10 N·m (89 lb in).

4. Install the oil pan scraper.
5. Install the oil pan scraper bolts.

Tighten
Tighten the oil pan scraper bolts to 10 N·m (89 lb in).

6. Install the oil pan. Refer to Oil Pan Replacement.