For 1990-2009 cars

## Battery Negative Cable Replacement LY7

### Removal Procedure

Important:

• | Always use replacement cables that are of the same type, diameter and length of the cables that you are replacing.

• | Always route the replacement cable the same way as the original cable.

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Disconnect the instrument panel (I/P) harness electrical connector (1) from the battery current sensor.
3. Remove the bolt (1) securing the negative battery cable to the side rail.
4. Disconnect the body harness connector (3) from the negative battery cable.
5. Remove the stud securing the negative battery cable to the engine block.
6. Lower the vehicle.
7. Remove the negative battery cable.

### Installation Procedure

1. Install and position the negative battery cable.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the negative battery cable to engine block stud.

Tighten
Tighten the stud to 50 N·m (37 lb ft).

3. Install the bolt (1) securing the negative battery cable to the side rail.

Tighten
Tighten the bolt to 36 N·m (27 lb ft).

4. Connect the body harness connector (3) to the negative battery cable.
5. Connect the I/P harness electrical connector (1) to the battery current sensor.
6. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.

## Battery Negative Cable Replacement LH2

### Removal Procedure

Important:

• | Always use replacement cables that are of the same type, diameter and length of the cables that you are replacing.

• | Always route the replacement cable the same way as the original cable.

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the fuel injector sight shield. Refer to Fuel Injector Sight Shield Replacement.
3. Disconnect the instrument panel (I/P) harness electrical connector (1) from the battery current sensor.
4. Disconnect the cable retaining clip from the stud on the shock tower.
5. Remove the bolt securing the negative battery cable to the shock tower.
6. Disconnect the instrument panel harness connector from the negative battery cable.
7. Disconnect the cable retaining clips from the engine bracket.
8. Remove the bolt securing the negative battery cable to the engine block.
9. Remove the negative battery cable.

### Installation Procedure

1. Position the negative battery cable to the engine.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the bolt securing the negative battery cable to the engine block.

Tighten
Tighten the bolt to 25 N·m (18 lb ft).

3. Connect the cable retaining clips to the engine bracket.
4. Connect the instrument panel harness connector to the negative battery cable.
5. Install the bolt securing the negative battery cable to the shock tower.

Tighten
Tighten the bolt to 10 N·m (89 lb in).

6. Connect the cable retaining clip to the stud on the shock tower.
7. Connect the I/P harness electrical connector (1) to the battery current sensor.
8. Install the fuel injector sight shield. Refer to Fuel Injector Sight Shield Replacement.
9. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.