For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Manual Shaft Detent Lever Hub Pin Notice: Refer to Pin Reuse Notice in the Preface section.
2 | Manual Shift Shaft Pin Notice: Refer to Pin Reuse Notice in the Preface section.
3 | Manual Shift Shaft Notice: Ensure the manual shift shaft seal is replaced before installing the shaft. Installing the seal after the shaft may cause damage to the seal, resulting in fluid leaks and transmission damage. Tip Refer to Manual Shift Shaft Seal Replacement .
4 | Manual Shaft Detent Lever Assembly
5 | Park Pawl Actuator Assembly
6 | Park Pawl Actuator Guide Pin Notice: Refer to Pin Reuse Notice in the Preface section. Tip Use a large pair of side cutters to "walk" the pin out.
7 | Park Pawl Actuator Guide
8 | Park Pawl Actuator Guide (O-ring) Seals Notice: Refer to Seal Reuse Notice in the Preface section.
9 | Park Pawl Tip Inspect for damage only. Do not remove. The park pawl is not a serviceable component.
10 | Park Pawl Spring Tip Inspect for damage only. Do not remove. The park pawl spring is not a serviceable component.
11 | Park Pawl Shaft Hole Plug

#### Special Tools

DT 47770 Seal Installer