For 1990-2009 cars

#### Special Tools

• | J 39232 Wiper Linkage Separator

• | J 39529 Wiper Linkage Installer

### Removal Procedure

1. Remove the wiper motor module assembly (1). Refer to Windshield Wiper System Module Replacement .
2. Remove the drive links from the wiper motor crank arm to the wiper motor using the J 39232 .
3. Remove the 3 screws (1) retaining the wiper motor to the wiper motor module.
4. Remove the wiper motor.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the wiper motor onto the wiper motor module assembly with the screws (1).

Tighten
Tighten the screws to 10 N·m (89 lb in).

2. Install the drive links onto the wiper motor crank arm using the J 39529 .
3. Install the wiper motor module assembly (1). Refer to Windshield Wiper System Module Replacement .
4. Operate the wiper and inspect for normal operation.