For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the front seats. Refer to Driver or Passenger Seat Replacement .
2. Remove the front seat cushion . Refer to Driver or Passenger Seat Cushion Ventilation Heating and Cooling Blower Replacement .
3. Recalibrate SIR passenger pressence system. After any parts of seat cushion or passenger presence system is removed, refer to Inflatable Restraint Sensing and Diagnostic Module Programming and Setup .

1 | Front Seat Back Frame Retaining Bolt (Qty: 4) Notice: Refer to Fastener Notice in the Preface section. Tighten 30 N·m (22 lb ft)
2 | Front Seat Adjuster Tip Disconnect the electrical connector and remove the front seat adjuster.