For 1990-2009 cars

Important: The following steps must be completed before using the symptom tables:

• | Refer to Diagnostic Starting Point - Vehicle .

- | There are no DTCs set.

- | The control modules can communicate via the serial data link.

• | Review the system operation in order to familiarize yourself with the system functions. Refer to Steering Wheel and Column Description and Operation .

### Visual/Physical Inspection

• | Inspect for aftermarket devices which could affect the operation of the tilt/telescoping steering column or the steering wheel theft deterrent lock system. Refer to Checking Aftermarket Accessories .

• | Inspect the easily accessible or visible system components for obvious damage or conditions which could cause the symptom.

### Intermittent

Faulty electrical connections or wiring may be the cause of intermittent conditions. Refer to Testing for Intermittent Conditions and Poor Connections .

### Symptom List

Refer to Steering Column Tilt/Telescoping Inoperative in order to diagnose the symptom.