For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
DEFINITION: Lead/pull is the deviation of the vehicle from a straight path on a level road with no pressure on the steering wheel.
1 | Did you perform the Vehicle Leads/Pull diagnostic table in Suspension General Diagnosis? | Go to Step 2 | Go to Vehicle Leads/Pulls
2 | Road test the vehicle to verify the concern. Select a smooth level surface to perform the test. Does the condition exist? | Go to Step 3 | System OK
3 | Cross-switch the front tire and wheel assemblies. Did you complete the procedure? | Go to Step 4 | --
4 | Does the vehicle lead/pull in the opposite direction? | Go to Step 5 | Go to Wheel Alignment Measurement
5 | Replace the tire that is pulling in the opposite direction and then install it to its original position. Refer to Tire Dismounting and Mounting . Did you complete the replacement? | Go to Step 6 | --
6 | Verify proper vehicle operation. Does the original condition still exist? | Go to Step 1 | System OK