For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the front seats. Refer to Driver or Passenger Seat Replacement .
2. Remove the front seat cushion retaining nuts. Refer to Driver or Passenger Seat Back Ventilation Heating and Cooling Blower Replacement .
3. Re-zero the inflatable restraint passenger presence system whenever the seat cushion or any component of the passenger presence system is removed. Refer to Passenger Presence System Programming and Setup .

1 | Seat Cushion Frame Refer to Driver or Passenger Seat Back Ventilation Heating and Cooling Blower Replacement .
2 | Front Seat Control Module Retaining Bolt (Qty: 3) Notice: Refer to Fastener Notice in the Preface section. Tighten 2N·m (18 lb in)
3 | Front Seat Control Module Tip Reprogram memory seat module when replacing the seat control module.