For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
ABS Module Retaining Nuts | 8 N·m | 71 lb in
Brake Line to Brake Hose Fitting | 27 N·m | 20 lb ft
Brake Pipe Bracket to Body Retaining Nuts | 10 N·m | 89 lb in
ECM Bracket Retaining Bolts | 9 N·m | 80 lb in
ECM Bracket Retaining Nuts | 12 N·m | 106 lb in
ECM to Bracket Retaining Nuts | 12 N·m | 106 lb in
Engine Mount Lower Retaining Nuts | 80 N·m | 59 lb ft
Front Frame to Body Front Mounting Bolts (Position 3) | 250 N·m | 185 lb ft
Front Frame to Body Mounting Bolts | 200 N·m | 147 lb ft
Front Frame to Body Rear and Mid Mounting Bolts (Positions 1 and 2) | 200 N·m | 147 lb ft
Intermediate Shaft to Steering Gear Retaining Bolt | 45 N·m | 35 lb ft
Outer Tie Rod to Steering Knuckle Retaining Nuts | 82 N·m | 60 lb ft
Outer Transmission Mounting Bolts | 60 N·m | 44 lb ft
Power Steering Gear Cooler to Air Conditioner Condenser Retaining Bolts | 9 N·m | 80 lb in
Power Steering Hose to Frame Retaining Bolts | 4 N·m | 35 lb in
Power Steering Pipes to Power Steering Gear Retaining Bolts | 23 N·m | 17 lb ft
Rear Frame to Body Front Mounting Bolts | 277 N·m | 204 lb ft
Rear Frame to Body Rear Mounting Bolts | 198 N·m | 146 lb ft
Rear Shock Absorber Lower Mounting Bolts | 165 N·m | 121 lb ft
Trailer Hitch Mounting Bolts | 95 N·m | 70 lb ft
Transmission Mount Lower Mounting Nuts | 60 N·m | 44 lb ft
Lower Ball Joint Retaining Nuts | 84 N·m | 62 lb ft
Washer Bottle to Steering Knuckle Retaining Bolts | 6 N·m | 53 lb in
Yoke to Shock Absorber Retaining Nut | 180 N·m | 133 lb ft