For 1990-2009 cars

### Removal Procedure

1. Remove the left quarter window trim panel. Refer to Sail Panel Replacement.
2. Disconnect the electrical connector.
3. Remove the bolt (1) securing the antenna module to the vehicle.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the bolt (1) securing the antenna module to the vehicle.

Tighten
Tighten the bolt (1) to 9 N·m (80 lb in).

2. Install the left quarter window trim panel. Refer to Sail Panel Replacement.