For 1990-2009 cars

### Removal Procedure

1. Remove the front console end panel. Refer to Front Floor Console Side Trim Rear Panel Replacement .
2. Remove the bolts securing the air outlet, and remove the air outlet.
3. Remove the bolts securing the wood grain trim panel to the housing.
4. Separate the wood grain trim panel from the housing.
5. Remove the screws securing the clock.
6. Remove the clock.

### Installation Procedure

1. Install the clock to the wood grain trim panel. Tighten the retaining screws.
2. Install the wood grain panel, and tighten the screws.
3. Install the air outlet and tighten the retaining screws.
4. Install the front console end panel. Refer to Front Floor Console Side Trim Rear Panel Replacement .