For 1990-2009 cars

### Circuit Description

The keyless entry antenna-right is located in the right hand door pull handle and is used as a short range low frequency (LF) antenna. As a vehicle with locked doors is approached with a valid keyless entry transmitter, and the exterior door handle is pulled, the keyless entry antenna broadcasts a challenge to the transmitter in approximately 1 meter range. If the response from the transmitter via radio frequency (RF) is valid, the locked door will be passively unlocked/unlatched and allow the door to be opened.

### DTC Descriptor

This diagnostic procedure supports the following DTC:

DTC B3120 Keyless Entry Antenna 2 Performance

This vehicle has DTCs which include DTC Symptoms. For more information on DTC Symptoms, refer to DTC Symptom Description .

DTC Symptom | DTC Symptom Descriptor
--- | ---
02 | Short to Ground
05 | Short to Battery or Open

### Conditions for Setting the DTC

The remote control door lock receiver (RCDLR) will set this DTC during antenna authentication if the keyless entry antenna-right is open, shorted to battery positive voltage, or shorted to ground. The RCDLR can only set a DTC when the vehicle system voltage is between 9-16 volts.

### Action Taken When the DTC Sets

The RCDLR will set and store DTC B3120 Keyless Entry Antenna 2 Performance.

### Conditions for Clearing the DTC

• | The RCDLR no longer detects an open, a short to power, or a short to ground on the antenna circuit.

• | Use the scan tool.

### Test Description

The numbers below refer to the step numbers on the diagnostic table.

1. Check to see if DTC B3120 is current.

2. Check if the passenger door handle operates properly. A valid input from the passenger door handle is required by the RCDLR to authenticate the antenna.

3. Testing for power and ground to the keyless entry antenna.

Step | Action | Yes | No
--- | --- | --- | ---
Schematic Reference: Remote Function Schematics Connector End View Reference: Remote Function Connector End Views
1 | Did you perform the Diagnostic System Check - Vehicle? | Go to Step 2 | Go to Diagnostic System Check - Vehicle
2 | Important: To achieve service by pass mode, ignition ON engine OFF, a programmed key fob must be detected within the passenger compartment of the vehicle.

1. Install the scan tool.
2. Push and hold the ACC button for 5 seconds to achieve the service bypass mode, with the engine OFF.
3. Select display DTCs function on the scan tool in the remote control door lock receiver (RCDLR) menu.

Does the scan tool display the DTC B3120 set as current?

Go to Step 3

Go to Testing for Intermittent Conditions and Poor Connections

3 |

1. With the scan tool, observe the passenger door handle parameter in the passenger door module (DDM) data list.
2. Activate the passenger exterior door handle.

Does the passenger door handle state display INACTIVE?

Go to Power Door Latch Inoperative - Passenger Door

Go to Step 4

4 | Important:

• | The voltage signal sent by the remote control door lock receiver (RCDLR) to the passive antenna is an AC voltage signal. The DMM must be set on AC voltage setting to record the voltage pulse to the passive antenna.

• | Use a DMM to record the voltage pulse using the MIN MAX setting to capture the A/C voltage pulse to the passive antenna.

1. Disconnect the keyless entry antenna-left at the right hand exterior door handle.
2. With the DMM, measure/capture for an AC voltage signal between the keyless entry antenna signal circuit and the low reference circuit.
3. With the scan tool, go to the RCDLR Special Functions menu. Select the Right Door Handle Antenna.
4. Use the scan tool to authenticate the antenna.

Was an A/C voltage signal captured on the DMM?

Go to Step 7

Go to Step 5

5 | Test both the keyless entry antenna signal and low reference circuit for an open. Refer to Circuit Testing and Wiring Repairs . Did you find and correct the condition? | Go to Step 12 | Go to Step 6
6 | Inspect for poor connections at the RCDLR. Refer to Testing for Intermittent Conditions and Poor Connections and Connector Repairs . Did you find and correct the condition? | Go to Step 12 | Go to Step 8
7 | Inspect for poor connections at the keyless entry antenna - right. Refer to Testing for Intermittent Conditions and Poor Connections and Connector Repairs . Did you find and correct the condition? | Go to Step 12 | Go to Step 10
8 | Test the keyless entry antenna signal circuit for a short to ground. Refer to Circuit Testing and Wiring Repairs . Did you find and correct the condition? | Go to Step 12 | Go to Step 9
9 | Replace the RCDLR. Refer to Control Module References for replacement, setup, and programming. Did you complete the replacement? | Go to Step 12 | --
10 | Test both the keyless entry antenna signal and low reference circuit for a short to power. Refer to Circuit Testing and Wiring Repairs . Did you find and correct the condition? | Go to Step 12 | Go to Step 11
11 | Replace the keyless entry antenna - right. Refer to Front Side Door Outside Handle Replacement . Did you complete the replacement? | Go to Step 12 | --
12 |

1. Clear the DTCs with the scan tool.
2. Operate the vehicle under conditions when DTC runs as specified in supporting documents.

Does the DTC set again?

Go to Step 3

System OK