For 1990-2009 cars

### Removal Procedure

1. Remove the right intake camshaft actuator (4). Refer to Camshaft Position Actuator Replacement - Bank 1 (Right Side) Intake .
2. Remove the right exhaust camshaft actuator (10). Refer to Camshaft Position Actuator Replacement - Bank 1 (Right Side) Exhaust .
3. Remove the right intake camshaft. Refer to Intake Camshaft Removal - Right Side .
4. Remove the right exhaust camshaft. Refer to Exhaust Camshaft Removal - Right Side .
5. Clean and inspect the camshafts. Refer to Camshaft Cleaning and Inspection .

### Installation Procedure

1. Install the right exhaust camshaft. Refer to Exhaust Camshaft Installation - Right Side .
2. Install the right intake camshaft. Refer to Intake Camshaft Installation - Right Side .
3. Install the right exhaust camshaft actuator (10). Refer to Camshaft Position Actuator Replacement - Bank 1 (Right Side) Exhaust .
4. Install the right intake camshaft actuator (4). Refer to Camshaft Position Actuator Replacement - Bank 1 (Right Side) Intake .