For 1990-2009 cars

### Removal Procedure

1. Remove the air inlet assembly. Refer to Air Inlet Assembly Replacement .
2. Remove the right air temperature actuator screws (1).
3. Remove the right air temperature actuator.
4. Disconnect the right air temperature actuator electrical connector.

### Installation Procedure

1. Connect the right air temperature actuator electrical connector.
2. Install the right air temperature actuator.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the right air temperature actuator screws (1).

Tighten
Tighten the screws to 1 N·m (9 lb in).

4. Install the air inlet assembly. Refer to Air Inlet Assembly Replacement .