For 1990-2009 cars

### Removal Procedure

Note:

• | There is no service interval for fuel filter replacement. Only replace the fuel filter if the filter is restricted.

• | If you find a restricted fuel filter, inspect and clean the inside of the fuel tank.

1. Relieve the fuel system fuel pressure. Refer to Fuel Pressure Relief.
2. Raise the vehicle. Refer to Lifting and Jacking the Vehicle.
3. Remove the rear suspension bracket. Refer to Differential Replacement.
4. Disconnect the quick-connect fittings (3 and 4) at the fuel filter inlet. Refer to Metal Collar Quick Connect Fitting Service or Plastic Collar Quick Connect Fitting Service.
5. Disconnect the threaded fitting (1) at the fuel filter outlet.
6. Drain any remaining fuel into an approved gasoline container.
7. Remove the fuel filter (2).
8. Remove the fuel pipe O-ring.
9. Discard the fuel filter into an approved container.

### Installation Procedure

1. Remove the protective caps from the new fuel filter.
2. If originally equipped, install new plastic connector retainers on the fuel filter inlets. Install the new retainers in the same position as on the old fuel filter.
3. Lubricate the new fuel pipe O-ring with clean engine oil.
4. Install the fuel pipe O-ring.
5. Slide the fuel filter into place.
6. Connect the quick-connect fittings (3 and 4) to the inlet side of the filter. Refer to Metal Collar Quick Connect Fitting Service or Plastic Collar Quick Connect Fitting Service.

Caution: Refer to Fastener Caution in the Preface section.

7. Connect the threaded fitting to the fuel filter outlet. Use a back-up wrench in order to prevent the fuel filter from turning.

Tighten
Tighten the fuel filter outlet fitting to 30 N·m (22 lb ft).

8. Install the rear suspension bracket. Refer to Differential Replacement.
9. Lower the vehicle.
10. Ensure that the fuel tank filler cap is installed correctly.
11. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
12. Perform the following procedure in order to inspect for leaks:

12.1. | Turn the ignition ON, with the engine OFF for 2 seconds.

12.2. | Turn the ignition OFF for 10 seconds.

12.3. | Turn the ignition ON without the engine OFF.

12.4. | Inspect for fuel leaks.

13. Install the fuel injection sight shield. Refer to Fuel Injector Sight Shield Replacement.