For 1990-2009 cars

Caution: Do not insert test equipment probes (DMM etc.) into any connector or fuse block terminal. The diameter of the test probes will deform most terminals. A deformed terminal will cause a poor connection, which will result in a system failure. Always use the J-35616 GM-Approved Terminal Test Kit in order to front probe terminals. Do not use paper clips or other substitutes to probe terminals.

When using the J-35616 GM-Approved Terminal Test Kit, ensure the terminal test adapter choice is the correct size for the connector terminal. Do not visually choose the terminal test adapter because some connector terminal cavities may appear larger than the actual terminal in the cavity. Using a larger terminal test adapter will damage the terminal. Refer to the J-35616 GM-Approved Terminal Test Kit label on the inside of the J-35616 GM-Approved Terminal Test Kit for the correct adapter along with the connector end view for terminal size.

The following procedure measures the voltage at a selected point in a circuit.

1. Set the rotary dial of the DMM to the V (DC) position.
2. Connect the positive lead of the DMM to one end of the circuit to be tested.
3. Connect the negative lead of the DMM to a good ground.
4. Turn the ignition switch to ON position, and allow all the accessories operative.
5. If the voltage measured is greater than 1 volt, there is a short to voltage in the circuit.