For 1990-2009 cars

1. Using a small screwdriver pry the wiring harness (55) off of the following components:

• | Pressure Control Solenoid (357)

• | TCC PWM Solenoid (352)

• | 1-2 Shift Solenoid (368)

• | 2-3 Shift Solenoid (369)

• | 4-5 Shift Solenoid (376)

• | Manual Shift Shaft Switch (602)

• | Input Speed Sensor (44)

• | Output Speed Sensor (42)

2. Remove the connector retainer (54) from the case (24).
3. Remove the wiring harness (55) from the case (24).