For 1990-2009 cars

Callout | Component Name
--- | ---
Front Side Marker Lamp Bulb Replacement Preliminary Procedure

1. Remove the front fascia assembly. Refer to Fascia, Extension, Reinforcement and Impact Bar Replacement - Front Bumper in Bumpers.
2. Remove the Headlamp assembly. Refer to Headlamps, Fog Lamps, Turn Signal Lamps, Side Marker Lamps Replacement - Front.

6 | Ballast Access Cover Screws Caution: Refer to Fastener Caution in the Preface section. Tighten: 3 N.m (27 lb in)
7 | Ballast Access Cover
9 | Front Side Marker Lamp Bulb Assembly