For 1990-2009 cars

Caution: Refer to Fastener Caution in the Preface section.

1. Install the engine front cover fitting.

Tighten
Tighten the engine front cover fitting to 25 N·m (18 lb ft).

2. Install the NEW thermostat gasket onto the thermostat.
3. Install the thermostat and gasket into the thermostat housing.
4. Install the thermostat housing.
5. Install the thermostat housing bolts.

Tighten
Tighten the thermostat housing bolts to 10 N·m (89 lb in).

6. Install the NEW water pump O-ring.
7. Install the water pump.
8. Install the water pump bolts.

Tighten
Tighten the water pump bolts to 10 N·m (89 lb in).