For 1990-2009 cars

Table 1: | Amplifier (AMP)
Table 2: | Dash Integration Module (DIM)
Table 3: | Digital Radio Receiver (DRR)
Table 4: | Driver Door Switch
Table 5: | Drivers Door Module
Table 6: | Engine Control Module (ECM) 3.6L (LY7)
Table 7: | Engine Control Module (ECM) 4.6L (LH2)
Table 8: | Instrument Panel Cluster (IPC)
Table 9: | Left Rear Door Module
Table 10: | Memory Seat Module (MSM)
Table 11: | Right Rear Door Module
Table 12: | Rear Integration Mode (RIM)
Table 13: | Rear Seat Module
Table 14: | Vehicle Theft Deterrent (VTD)
Table 15: | Passenger Door Module
Table 16: | Sensing Diagnostic Module (SDM)
Table 17: | Transmission Control Module (TCM)

#### Amplifier (AMP)

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Operating Conditions: Ignition ON/Engine Running
Battery Voltage | Engine Electrical | Volts | 13.9 Volts

#### Dash Integration Module (DIM)

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Operating Conditions: Ignition OFF/Engine Running
Battery Voltage | Data Display | Volts | 13.9 Volts

#### Digital Radio Receiver (DRR)

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Operating Conditions: Ignition ON/Engine Running
Battery Voltage | Data Display | Volts | 13.9 Volts

#### Driver Door Switch

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Operating Conditions: Ignition ON/Engine Running
Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
Battery Voltage | Data Display | Volts | 13.9 Volts

#### Drivers Door Module

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Operating Conditions: Ignition ON/Engine Running
Battery Voltage | Data Display | Volts | 13.9 Volts

#### Engine Control Module (ECM) 3.6L (LY7)

San Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Operating Conditions: Ignition ON/Engine OFF
Crank Request Signal | Electrical | Yes/No | No
GEN F-Terminal Signal | Electrical/Theft Deterrent Data | % | 0%
GEN L-Terminal Signal Command | Electrical/Theft Deterrent Data | % | Varies
Ignition 1 Signal | Electrical/Theft Deterrent Data | 0-25.5 V | 12.8-14.2 V
Ignition 1 Signal | Electrical/Theft Deterrent Data | On/Off | Off
Park/Neutral Position Switch | Electrical/Theft Deterrent Data | Park/Neutral/In Gear | Park
Starter Relay Command | Electrical/Theft Deterrent Data | On/Off | Off
Starter Relay Circuit Status | Electrical/Theft Deterrent Data | Fault/Indeterminate/OK | OK
APP Indicated Angle | Electrical/Theft Deterrent Data | 0-100% | 0.0
ECT Sensor | Electrical/Theft Deterrent Data | °C/°F | Varies
Brake Pedal Signal Status | Electrical/Theft Deterrent Data | Valid/Invalid | Valid
Clutch Start Switch (If equipped) | Electrical/Theft Deterrent Data | Applied/Released | Depending on clutch pedal position
EC Ignition Relay Circuit | Electrical/Theft Deterrent Data | OK/Faulty/Indeterminate | OK
EC Ignition Relay Command | Electrical/Theft Deterrent Data | On/Off | ON
EC Ignition Relay Feedback Signal | Electrical/Theft Deterrent Data | 0-25.5 V | 12.0-14.5 V
Engine Oil Pressure Sensor | Electrical/Theft Deterrent Data | kPa (psi) | Varies
Engine Speed | Electrical/Theft Deterrent Data | RPM | 650 RPM
Ignition 0 Signal | Electrical/Theft Deterrent Data | On/Off | ON
Initial Brake Apply Signal | Electrical/Theft Deterrent Data | Applied/Released | Released
MIL Requested by DTC | Electrical/Theft Deterrent Data | Yes/No | No
Stop Lamp Pedal Switch | Electrical/Theft Deterrent Data | Applied/Released | Released
System Power Mode | Electrical/Theft Deterrent Data | Off, Accessory, RAP, Run, or Crank Request | Run
Vehicle Speed Sensor | Electrical/Theft Deterrent Data | km/miles | Varies

#### Engine Control Module (ECM) 4.6L (LH2)

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Operating Conditions: Ignition ON/Engine OFF
Crank Request Signal | Electrical/Theft Deterrent Data | Yes/No | No
GEN F-Terminal Signal | Electrical/Theft Deterrent Data | % | %
GEN L-Terminal Circuit Status | Electrical/Theft Deterrent Data | OK/Incomplete/Short to B+/Short to Ground/Open | OK
GEN L-Terminal Signal Command | Electrical/Theft Deterrent Data | % | 0%
Ignition 1 Signal | Electrical/Theft Deterrent Data | Volts | Varies
Park/Neutral Position Switch | Electrical/Theft Deterrent Data | Park/Neutral/In Gear | Park
Starter Relay Command | Electrical/Theft Deterrent Data | On/Off | Off
Starter Relay Circuit Status | Electrical/Theft Deterrent Data | Fault/Indeterminate/OK | OK
APP Indicated Angle | Electrical/Theft Deterrent Data | 0-100% | 0.0
BPP Circuit Signal | Electrical/Theft Deterrent Data | Applied/Released | Released
BPP Signal | Electrical/Theft Deterrent Data | Applied/Released/Invalid | Released
EC Ignition Relay Circuit Status | Electrical/Theft Deterrent Data | OK/Incomplete/Short to B+/Short to Ground/Open | OK
EC Ignition Relay Command | Electrical/Theft Deterrent Data | On/Off | On
EC Ignition Relay Feedback Signal | Electrical/Theft Deterrent Data | Volts | 13.5 V
ECT Sensor | Electrical/Theft Deterrent Data | °C/°F | Varies
Engine Oil Pressure Sensor | Electrical/Theft Deterrent Data | kPa/psi | Varies
Engine Speed | Electrical/Theft Deterrent Data | RPM | 650 RPM
Ignition Accessory Signal | Electrical/Theft Deterrent Data | On/Off | On
MIL Requested by DTC | Electrical/Theft Deterrent Data | Yes/No | No
Remote Vehicle Start (RVS) Disabled, History DTC (1-8) | Electrical/Theft Deterrent Data | Vehicle Remote Start Disabled (Reason) | Varies
Remote Vehicle Start (RVS) Request Signal | Electrical/Theft Deterrent Data | Yes/No | No
Vehicle Speed Sensor | Electrical/Theft Deterrent Data | km/miles | Varies

#### Instrument Panel Cluster (IPC)

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Operating Conditions: Ignition ON/Engine Running
Battery Voltage | Data Display | Volts | 13.9 Volts

#### Left Rear Door Module

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Operating Conditions: Ignition ON/Engine Running
Battery Voltage | Data Display | Volts | 13.9 Volts

#### Memory Seat Module (MSM)

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Operating Conditions: Ignition ON/Engine Running
Battery Voltage | Data Display | Volts | 13.9 Volts

#### Right Rear Door Module

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Operating Conditions: Ignition ON/Engine Running
Battery Voltage | Data Display | Volts | 13.9 Volts

#### Rear Integration Mode (RIM)

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Operating Conditions: Ignition ON/Engine Running
Battery Voltage | Data Display | Volts | 13.9 Volts

#### Rear Seat Module

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Operating Conditions: Ignition ON/Engine Running
Battery Voltage | Data Display | Volts | 13.9 Volts

#### Vehicle Theft Deterrent (VTD)

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Operating Conditions: Ignition ON/Engine Running
Battery Voltage | Data Display | Volts | 12.0 Volts
Start Disabled | Data Display | Yes/No | Yes

#### Passenger Door Module

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Operating Conditions: Ignition ON/Engine Running
Battery Voltage | Data Display | Volts | 13.9 Volts

#### Sensing Diagnostic Module (SDM)

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Operating Conditions: Ignition ON/Engine Running
Battery Voltage | Data Display | Volts | 13.9 Volts

#### Transmission Control Module (TCM)

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Operating Conditions: Ignition ON/Transmission in Park
IMS | Engine Electrical | Park, Park/Reverse, Reverse, Reverse/Neutral, Neutral, Neutral/Drive 4, Drive 4, Drive 4/Drive 3, Drive 3, Drive 3/Drive 2, Drive 2, Drive 2/Drive 1, Drive 1, INVALID, OPEN | Park