For 1990-2009 cars

### Removal Procedure

1. Turn the ignition OFF.
2. Remove the fuel injector sight shield. Refer to Fuel Injector Sight Shield Replacement .
3. Disconnect the manifold absolute pressure (MAP) sensor electrical connector.
4. Remove the bolt (1) and bracket (2) from the MAP sensor (3).
5. Remove the MAP sensor (3).
6. Inspect the MAP sensor seal for wear or damage. If a problem is found, replace as necessary.

### Installation Procedure

1. Install the MAP sensor (3).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the bracket (2) and bolt (1).

Tighten
Tighten the bracket bolt to 12 N·m (106 lb in).

3. Connect the MAP sensor electrical connector.
4. Install the fuel injector sight shield. Refer to Fuel Injector Sight Shield Replacement .