For 1990-2009 cars

## Engine Mount Bracket Replacement - Right Side w/AWD

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the right exhaust manifold. Refer to Exhaust Manifold Removal - Right Side .
3. Install a screw jack with a block of wood under the oil pan for support.
4. Remove the right engine mount upper retaining nut.

Important: Ensure not to distort or bend the engine mount bracket mounting bolts.

5. Remove the right engine mount bracket mounting bolts.
6. Remove the engine mount bracket from the vehicle.

### Installation Procedure

1. Install the engine mount bracket to the vehicle.

Notice: Refer to Fastener Notice in the Preface section.

2. Tighten the engine mount bracket mounting bolts.

Tighten
Tighten the bolts to 60 N·m (44 lb ft).

3. Tighten the M8 engine mount bracket mounting bolt.

Tighten
Tighten the bolts to 38 N·m (28 lb ft).

4. Remove the screw jack.
5. Install the upper engine mount retaining nut.

Tighten
Tighten the nut to 80 N·m (59 lb ft).

6. Install the right exhaust manifold. Refer to Exhaust Manifold Replacement - Right Side .

Tighten
Tighten the nut to 80 N·m (59 lb ft).

7. Lower the vehicle.

## Engine Mount Bracket Replacement - Right Side w/RWD

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Install a screw jack with a block of wood under the oil pan for support.
3. Remove the lower engine mount retaining nut.
4. Raise the engine using the screw jack until the weight is removed from the mount.
5. Remove the upper engine mount retaining nut.
6. Remove the engine mount from the vehicle.
7. Remove the starter. Refer to Starter Motor Replacement .

Important: Ensure not to distort or bend the engine mount heat shield.

8. Remove the right engine mount bracket mounting bolts.
9. Remove the engine mount bracket from the vehicle.

### Installation Procedure

1. Install the engine mount bracket to the vehicle.

Notice: Refer to Fastener Notice in the Preface section.

2. Tighten the engine mount bracket mounting

Tighten
Tighten the bolts to 60 N·m (44 lb ft).

3. Install the starter. Refer to Starter Motor Replacement .
4. Install the engine mount to the vehicle.
5. Install the upper engine mount retaining nut.

Tighten
Tighten the nut to 80 N·m (59 lb ft).

6. Lower the engine using the jack screw until the weight is resting on the mount.
7. Install the engine mount retaining nut.

Tighten
Tighten the nut to 80 N·m (59 lb ft).

8. Remove the screw jack and block of wood from under the oil pan.
9. Lower the vehicle.