For 1990-2009 cars

### Removal Procedure

Caution: Refer to Exhaust Service Caution in the Preface section.

Caution: Refer to Protective Goggles and Glove Caution in the Preface section.

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the bolts securing the center bearing heat shield to the center bearing.
3. Remove the heat shield from the center bearing in the following order:

3.1. | Tilt the heat shield to either side.

3.2. | Slide the heat shield out from between the body, the drive shaft center bearing, and the exhaust pipes.

3.3. | Remove the heat shield from the vehicle.

### Installation Procedure

1. Install the center bearing heat shield to the center bearing in the following order:

1.1. | Slide the heat shield in between the body, the drive shaft center bearing, and the exhaust pipes.

1.2. | Align the holes in the heat shield with the holes in the center bearing.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the bolts securing the center bearing heat shield to the center bearing.

Tighten
Tighten the center bearing heat shield bolts to 8 N·m (71 lb in).

3. Lower the vehicle.