For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the left exhaust manifold. Refer to Exhaust Manifold Removal - Left Side.
3. Install a screw jack with a block of wood under the oil pan for support.
4. Remove the upper engine mount retaining nut.

Note: Ensure not to distort or bend the engine mount heat shield.

5. Remove the left engine mount bracket retaining bolts.
6. Remove the left engine mount bracket.

### Installation Procedure

1. Install the left engine mount brackets.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the left engine mount bracket retaining bolts.

Tighten
Tighten the bolts to 60 N·m (44 lb ft).

3. Install the upper engine mount retaining nut.

Tighten
Tighten the nut to 80 N·m (59 lb ft).

4. Remove the screw jack.
5. Install the left exhaust manifold. Refer to Exhaust Manifold Removal - Left Side.
6. Lower the vehicle.