For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Shift Control Knob Bezel Tip

• | Removal: Carefully insert a small flat bladed tool between the bezel (1) and the shift knob. Apply careful downward pressure to the bezel to separate the bezel from the shift knob.

• | Installation: Lift the bezel (1) up to the shift knob (3) until a click sound is heard indicating the bezel is secured to the shift knob.

2 | Shift Control Knob Screw Caution: Refer to Fastener Caution in the Preface section. Tip Loosen the shift control knob screw approximately 3-4 turns. It is not necessary to fully remove the screw from the shift control knob. Tighten
2 N·m (18 lb in)

3 | Shift Control Knob