For 1990-2009 cars

Callout | Component Name
--- | ---
1 | 4-5-6 Clutch Dampener Retaining Ring Notice: Ensure the retaining ring is fully seated when installed. Using a screwdriver, fully seat the retaining ring into the groove by pushing on the inside diameter around the whole circumference. If the retaining ring is not fully seated, transmission damage will result.
2 | 4-5-6 Clutch Dampener Apply Plate
3 | 4-5-6 Clutch Dampener Tip Dry and inspect the clutch dampener for the following conditions:

• | Pitting

• | Flaking

• | Delamination

• | Wear

• | Glazing

• | Cracking

If any of these conditions are found, replace the dampener.