For 1990-2009 cars

### Description

The engine control module (ECM) uses information from the crankshaft position (CKP) sensor and the camshaft position (CMP) sensors in order to determine when an engine misfire is occurring. By monitoring variations in the crankshaft rotation speed for each cylinder, the ECM is able to detect individual misfire events. A misfire rate that is high enough can cause 3-way catalytic converter damage. The malfunction indicator lamp (MIL) will flash ON and OFF when the conditions for catalytic converter damage are present. DTCs P0301 through P0306 correspond to cylinders 1 through 6. If the ECM is able to determine that a specific cylinder is misfiring, the DTC for that cylinder will set. If the misfire rate is sufficient to cause emission levels to exceed a predetermined value, this DTC sets.

### DTC Descriptor

This diagnostic procedure supports the following DTC:

DTC P0300 Engine Misfire Detected

### Conditions for Running the DTC

#### Conditions 1

• | DTCs P0121, P0122, P0123, P0221, P0222, P0223, P0335, P0336, or P0338 are not set.

• | The engine speed is between 400-7,000 RPM and steady.

• | The delivered torque signal is more than 12 percent at idle.

• | The delivered torque signal is between 10.5-29.3 percent with the transmission in drive.

• | The intake air temperature (IAT) is more than -30°C (-22°F).

• | The fuel level is more than 11.6 percent.

• | Or the fuel level is less than 11.6 percent and misfire MIL is turned ON.

• | Or fuel level scan tool DTC P0461, P0462, P0463, P2067, P2066 or P2068 have been set.

• | The antilock brake system/traction control system (ABS/TCS) is not active.

• | The ECM is not receiving a rough road signal.

• | The fuel cut-off is not active, including the traction control, the deceleration, the high vehicle speed, and the high engine speed.

• | The change in engine speed per second is less than 200-362 RPM.

• | The change in volumetric efficiency per round is less than 225-1,350 percent.

• | After start the engine, there is cylinder ignition at least 6times.

• | The clutch pedal press/release change has a problem.

• | The ECM detects that the fuel leaks test procedure has closed.

• | The engine reverse control system is inactive.

• | DTC P0300 runs continuously when the above conditions exist for at least 1000 engine revolutions.

#### Conditions 2

• | When a misfire rate high enough causes 3-way catalytic converter damage, the above conditions are met except for the follow:

• | The first test interval delays to 1000 engine revolutions.

• | The engine coolant temperature is less than 47°C (116.6°F).

• | The fuel level is more than 11.6 percent.

• | Or fuel level is less than 11.6 percent, the malfunction indicator lamp flashes not for the first time.

• | DTC P0300 runs continuously when the above conditions exist for at least 1000 engine revolutions.

### Conditions for Setting the DTC

• | The ECM detects a crankshaft rotation speed variation indicating a misfire rate of 1.82 percent, which is sufficient to cause emissions levels to exceed mandated standards.

| OR

• | The ECM detects a crankshaft rotation speed variation indicating a misfire rate of 1.81-5 percent, which is sufficient to cause 3-way catalytic converter damage.

• | The condition above exists for more than 4 seconds.

### Action Taken When the DTC Sets

• | The control module illuminates the malfunction indicator lamp (MIL) on the second consecutive ignition cycle that the diagnostic runs and fails.

• | The control module records the operating conditions at the time the diagnostic fails. The first time the diagnostic fails, the control module stores this information in the Failure Records. If the diagnostic reports a failure on the second consecutive ignition cycle, the control module records the operating conditions at the time of the failure. The control module writes the operating conditions to the Freeze Frame and updates the Failure Records.

### Conditions for Clearing the MIL/DTC

• | The control module turns OFF the malfunction indicator lamp (MIL) after 4 consecutive ignition cycles that the diagnostic runs and does not fail.

• | A current DTC, last test failed, clears when the diagnostic runs and passes.

• | A history DTC clears after 40 consecutive warm-up cycles, if no failures are reported by this or any other emission related diagnostic.

• | Clear the MIL and the DTC with a scan tool.

### Diagnostic Aids

• | A misfire DTC could be caused by an excessive vibration from sources other than the engine. Inspect for the following possible sources:

- | A tire or wheel that is out of round or out of balance

- | Variable thickness brake rotors

- | An unbalanced drive shaft

- | Certain rough road conditions

- | A damaged accessory drive component or belt

• | A misfire DTC could be caused by a camshaft actuator stuck in the full advance or retard position.

• | For an intermittent condition, refer to Intermittent Conditions .

### Test Description

The numbers below refer to the step numbers on the diagnostic table.

1. This step determines if there is a current condition.

2. If the Misfire Current Counters are incrementing, but the engine is NOT misfiring, this indicates a mechanical condition. For example, an accessory drive belt could cause this condition.

#### DTC P0300 - Engine Misfire Detected

Step | Action | Yes | No
--- | --- | --- | ---
1 | Did you perform the Diagnostic System Check - Vehicle? | Go to Step 2 | Go to Diagnostic System Check - Vehicle
2 | Important: The engine may only misfire when the engine is under a load. An engine load may be necessary to verify the condition.

1. Start the engine.
2. Monitor the Misfire Current Cyl. 1-6 Counter parameters with a scan tool.

Are any of the Misfire Current Counters incrementing?

Go to Step 4

Go to Step 3

3 |

1. Observe the Freeze Frame/Failure Records for this DTC.
2. Turn OFF the ignition for 30 seconds.
3. Start the engine.
4. Operate the vehicle within the Conditions for Running the DTC. You may also operate the vehicle within the conditions that you observed from the Freeze Frame/Failure Records.

Did the DTC fail this ignition?

Go to Step 4

Go to Diagnostic Aids

4 | Is the engine misfiring? | Go to Step 5 | Go to Symptoms - Engine Mechanical
5 | Observe the DTC Info with a scan tool. Is DTC P0011, P0014, P0021, P0024, P0201-P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, P0277, P0335, P0336, P0338, P0351-P0356, P2088, P2090, P2092, P2094, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316 also set? | Go to Diagnostic Trouble Code (DTC) List - Vehicle | Go to Step 6
6 | Is there an engine mechanical noise? | Go to Symptoms - Engine Mechanical | Go to Step 7
7 | Is there more than one cylinder specific misfire DTC set? | Go to Step 8 | Go to DTC P0301-P0306
8 | Are there any heated oxygen sensor (HO2S) DTCs set? | Go to Diagnostic Trouble Code (DTC) List - Vehicle | Go to Step 9
9 |

1. Inspect or test for the following conditions:

• | Inspect the vacuum hoses for splits, kinks, and proper connections.

• | Inspect the throttle body and the intake manifold for vacuum leaks.

• | Inspect the crankcase ventilation valve and/or system for any vacuum leaks.

• | Test for the correct fuel pressure. Refer to Fuel System Diagnosis .

• | Inspect the fuel system for any restrictions, leaks or fuel contamination. Refer to Fuel System Diagnosis or Alcohol/Contaminants-in-Fuel Diagnosis .

• | Inspect for fouled or damaged spark plugs. Determine what caused the spark plugs to foul. Refer to Spark Plug Inspection .

• | Inspect the exhaust system for restrictions. Refer to Restricted Exhaust .

• | Inspect the engine control grounds for being clean, tight, and in the correct location.

• | Inspect for a camshaft actuator stuck in the full advance or retard position.

2. Repair as necessary.

Did you find and correct the condition?

Go to Step 10

Go to Symptoms - Engine Mechanical

10 |

1. Clear the DTCs with a scan tool.
2. Turn OFF the ignition for 30 seconds.
3. Start the engine.
4. Operate the vehicle within the Conditions for Running the DTC. You may also operate the vehicle within the conditions that you observed from the Freeze Frame/Failure Records.

Did the DTC fail this ignition?

Go to Step 2

Go to Step 11

11 | Observe the Capture Info with a scan tool. Are there any DTCs that have not been diagnosed? | Go to Diagnostic Trouble Code (DTC) List - Vehicle | System OK