For 1990-2009 cars

Callout | Component Name
--- | ---
Notice: Use Dexron VI transmission fluid only. Failure to use the proper fluid may result in transmission internal damage.

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Place a suitable drain pan under the transmission.

1 | Transmission Fluid Pan Bolt (Qty: 18) Notice: Refer to Fastener Notice in the Preface section. Tip Tighten the bolts in the sequence shown. Tighten
9 N·m (80 lb in)

2 | Transmission Fluid Pan Assembly Tip

• | Check the condition of the draining fluid. Refer to Transmission Fluid Check .

• | Fill the transmission with the proper fluid. Refer to Transmission General Specifications and Transmission Fluid Fill Procedure .

• | Fill the transmission with the proper amount of transmission fluid. Refer to Fluid Capacity Specifications and Transmission Fluid Check .

3 | Transmission Fluid Pan Gasket Tip The fluid pan gasket is reusable. Inspect the gasket to determine if it may be reused.
4 | Fluid Filter Assembly Tip

• | Pull the fluid filter assembly straight out. Do not bend or twist the filter neck.

• | Use a new fluid filter assembly.

5 | Fluid Filter Seal Assembly Notice: Do not damage the case sealing surface when removing the filter seal assembly. Tip

• | Use a screwdriver or snap ring pliers to remove the filter seal.

• | Use the DT 47848 and the J 42183 to install the filter seal.

• | Use a new fluid filter seal assembly.

• | Lubricate the filter seal with transmission fluid before installing the filter.

#### Special Tools

• | DT 47848 Seal Installer

• | J 42183 Driver Handle