For 1990-2009 cars

## Oil Filter Adapter Assemble With Oil Cooler

1. If removed, install the oil filter bypass valve (6).

Caution: Refer to Fastener Caution in the Preface section.

2. Install the oil filter fitting (5).

Tighten
Tighten the oil filter fitting to 29 N·m (21 lb ft).

3. Install a NEW O-ring (7) on the oil pressure switch (8).
4. Install the oil pressure switch (8).

Tighten
Tighten the oil pressure switch to 16 N·m (12 lb ft).

5. Install the heat shield (9).
6. Install the heat shield bolts (10).

Tighten
Tighten the heat shield bolts to 10 N·m (89 lb in).

7. Install the NEW oil filter adapter gasket (1).