For 1990-2009 cars

Name | 6L50
--- | ---
RPO Codes | MYB
Production Location | Strasbourg, France Ypsilanti, Michigan (USA)
Transmission Drive | Rear Wheel Drive
1st Gear Ratio | 4.065
2nd Gear Ratio | 2.371
3rd Gear Ratio | 1.551
4th Gear Ratio | 1.157
5th Gear Ratio | 0.853
6th Gear Ratio | 0.674
Reverse | 3.200
Torque Converter Size - Diameter of Torque Converter Turbine | 245/258 mm
Pressure Taps | Line Pressure
Transmission Fluid Type | DEXRON® VI
Transmission Type: 6 | Six Forward Gears
Transmission Type: L | Longitude Mount
Transmission Type: 50/80 | Product Series
Position Quadrant | P, R, N, D, M
Case Material | Die Cast Aluminum
Transmission Net Weight (Approximate) | 90 kg (198 lb)
Maximum Trailer Towing Capacity | Refer to applicable owner's manual.